{ XE "46-3.01C(1)\_N10-26-22\_\_2022" }

Page 1 of 1

Section 46-3.01C(1). Use to test verification test soil nails to 3 x T. Use with NSSP for section 46-3.01D(2)(b)(ii)(2).

Add at the end of section 46-3.01C(1):

Submit calculations that verify the size and tensile strength of verification test nail bar can provide nominal tensile resistance at least 1.5 times the maximum verification test load described in Verification Test Loading Schedule.