{ XE "46-2.01B\_N04-01-21\_\_2018" }

Page 1 of 1

Section 46-2.01B. Use for verification tests for ground anchors. Use with NSSPs for sections 46-2.01C, 46-2.01D(2)(c), 46-2.01D(3)(c), and 46-2.03E.

Add to section 42-2.01B:

**anchor bonded length:** length of grout/ground interface that provide verifiable pullout resistance using ground anchor verification test.

**anchor unbonded length:** length of ground anchor measured from the finish grade to the top of anchor bonded length.

**tendon bonded length:** length of ground anchor tendons bonded with surrounding grout.