{ XE "96-1.02T\_N03-29-21\_\_2018" }

Page 1 of

Section 96-1.02T. Use for lightweight fill using EPS geofoam blocks. Use with NSSPs for section 19-13 and 96-1.02S

Replace section 96-1.02T with:

### 96-1.02T Gasoline Resistant Geomembrane

1

Gasoline resistance geomembrane must comply with section 96-1.02R and must be:

1. Polyethylene

2. Gasoline and water resistant

3. Unreinforced or scrim reinforced

2

Gasoline resistant geomembrane must confine spilled liquid hydrocarbons, including gasoline, diesel fuel, kerosene, hydraulic fluid, methanol, ethanol, mineral spirits, and naphtha.