Page 1 of 1

Section 76-6. Use to present the wells to be destroyed in the Special Provisions, instead of in the supplemental project information.

Replace the second paragraph with:

1.

Before starting earthwork, destroy wells shown in the following table. For temporary wells installed during construction, destroy the wells.

|  |
| --- |
| Wells to be Destroyed |
| Well ID | Well Type | (Northing, Easting) | (Latitude, Longitude) | Depth (ft) | Diameter (in) | Casing Type | Time to Destroy |
|  | e.g., piezometer, slope inclinometer, TDR, Vibrating-wire transducer |  |  |  |  |  | e.g., after clearing and grubbing, after conclusion of pullout tests, when ordered |